<config configName="default" projectName="test1" configVersion="1.2" device="dsPIC33EV256GM102" deviceLibraryClass="com.microchip.mcc.mcu16.Mcu16PeripheralLibrary" coreVersion="5.8.2">
   <usedPackages class="java.util.ArrayList"/>
   <usedClasses class="java.util.TreeMap">
      <entry>
         <string>ADC1</string>
         <string>class com.microchip.mcc.mcu16.modules.adc_simsam.ADC</string>
      </entry>
      <entry>
         <string>DMT</string>
         <string>class com.microchip.mcc.mcu16.systemManager.dmt.DMT</string>
      </entry>
      <entry>
         <string>ICD</string>
         <string>class com.microchip.mcc.mcu16.systemManager.icd.Icd</string>
      </entry>
      <entry>
         <string>INTERNAL OSCILLATOR</string>
         <string>class com.microchip.mcc.mcu16.systemManager.clk.Clock</string>
      </entry>
      <entry>
         <string>Interrupt Module</string>
         <string>class com.microchip.mcc.mcu16.interruptManager_dsPIC.InterruptManager_dsPIC</string>
      </entry>
      <entry>
         <string>Main Manager</string>
         <string>class com.microchip.mcc.mcu16.mainManager.MainManager</string>
      </entry>
      <entry>
         <string>Pin Module</string>
         <string>class com.microchip.mcc.mcu16.pinManager.PinManager</string>
      </entry>
      <entry>
         <string>RESET</string>
         <string>class com.microchip.mcc.mcu16.systemManager.reset.RESET</string>
      </entry>
      <entry>
         <string>SPI1</string>
         <string>class com.microchip.mcc.mcu16.modules.spi.SPI</string>
      </entry>
      <entry>
         <string>System Module</string>
         <string>class com.microchip.mcc.mcu16.systemManager.DefaultSystemManagerMcu16</string>
      </entry>
      <entry>
         <string>TMR3</string>
         <string>class com.microchip.mcc.mcu16.modules.tmr.TMR</string>
      </entry>
      <entry>
         <string>WATCHDOG</string>
         <string>class com.microchip.mcc.mcu16.systemManager.wdt.Wdt</string>
      </entry>
      <entry>
         <string>com.microchip.mcc.boardsupportlibrary.BoardSuppportLibraryLibraryModule</string>
         <string>class com.microchip.mcc.protocolServices.base.modules.librarymodule.LibraryModule</string>
      </entry>
      <entry>
         <string>com.microchip.mcc.mcu16.Mcu16PeripheralLibraryLibraryModule</string>
         <string>class com.microchip.mcc.protocolServices.base.modules.librarymodule.LibraryModule</string>
      </entry>
   </usedClasses>
   <usedLibraries class="java.util.ArrayList">
      <ILibraryFile class="com.microchip.mcc.core.library.BaseLibraryFile" libraryClass="com.microchip.mcc.mcu16.Mcu16PeripheralLibrary" version="1.171.4"/>
      <ILibraryFile class="com.microchip.mcc.core.library.BaseLibraryFile" libraryClass="com.microchip.mcc.boardsupportlibrary.BoardSuppportLibrary" version="1.12.0"/>
   </usedLibraries>
   <tokenMap class="java.util.TreeMap">
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="ADC1_ADIISRFunction"/>
         <value>ISR_ADC1_ADI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="ADCFunctionMode"/>
         <value>ADC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN24"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN25"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN26"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN27"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN32"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN4"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="CTMU"/>
         <value>channel_CTMU</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="Internal Band Gap Reference"/>
         <value>channel_Internal Band Gap Reference</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="SCAN_ENABLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="Scan_Count"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="adcsCustomKey"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="localClockKey"/>
         <value>69093750</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="macroisr"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="tad"/>
         <value>1.30257E-7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NA" alias="AN1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NA" alias="VREFL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NB" alias="AN1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NB" alias="VREFL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN24"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN26"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN27"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN32"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN4"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN5"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="CTMU"/>
         <value>62</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="Internal Band Gap Reference"/>
         <value>61</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="OA1/AN3"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="OA2/AN0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="OA5/AN25"/>
         <value>25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN24"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN26"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN27"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN32"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN4"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN5"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="CTMU"/>
         <value>62</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="Internal Band Gap Reference"/>
         <value>61</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="OA1/AN3"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="OA2/AN0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="OA5/AN25"/>
         <value>25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123NA" alias="CH1=VREF-"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123NA" alias="CH1=VREF-,CH2=VREF-,CH3=VREF-"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123NA" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123NB" alias="CH1=VREF-"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123NB" alias="CH1=VREF-,CH2=VREF-,CH3=VREF-"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123SA" alias="CH1=OA1/AN3"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123SA" alias="CH1=OA1/AN3,CH2=AN4,CH3=AN5"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123SA" alias="CH1=OA1/AN3,CH2=OA2/AN0,CH3=OA3/AN6"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123SA" alias="CH1=OA1/AN3,CH2=OA2/AN0,CH3=OA5/AN25"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123SA" alias="CH1=OA2/AN0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123SA" alias="CH1=OA2/AN0,CH2=AN1,CH3=AN2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123SA" alias="CH1=OA2/AN0,CH2=OA5/AN25,CH3=OA3/AN6"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123SA" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123SB" alias="CH1=OA1/AN3"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123SB" alias="CH1=OA1/AN3,CH2=AN4,CH3=AN5"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123SB" alias="CH1=OA1/AN3,CH2=OA2/AN0,CH3=OA5/AN25"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123SB" alias="CH1=OA2/AN0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123SB" alias="CH1=OA2/AN0,CH2=AN1,CH3=AN2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ADON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ADON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ADSIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ADSIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ASAM" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ASAM" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="DMABM" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="DMABM" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="DONE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="DONE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="FORM" alias="Absolute decimal result, unsigned, right-justified"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="FORM" alias="Absolute fractional result, unsigned, left-justified"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="FORM" alias="Decimal result, signed, right-justified"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="FORM" alias="Fractional result, signed, left-justified"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="MODE12" alias="10-bit"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="MODE12" alias="12-bit"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SAMP" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SAMP" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SIMSAM" alias="Sequential"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SIMSAM" alias="Simultaneous"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="CTMU"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="Clearing sample bit ends sampling and starts conversion"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="INT0"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="Internal counter ends sampling and starts conversion"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="PWM Primary Special Event Trigger"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="PWM1 Primary Trigger"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="PWM2 Primary Trigger"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="PWM3 Primary Trigger"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="TMR3"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="TMR5"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRCG" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRCG" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="ALTS" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="ALTS" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="BUFM" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="BUFM" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="BUFS" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="BUFS" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="CHPS" alias="1 Channel"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="CHPS" alias="2 Channel"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="CHPS" alias="4 Channel"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="CSCNA" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="CSCNA" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="NVCFG0" alias="AVSS"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="PVCFG" alias="AVDD"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 10th sample/conversion operation"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 11th sample/conversion operation"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 12th sample/conversion operation"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 13th sample/conversion operation"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 14th sample/conversion operation"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 15th sample/conversion operation"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 16th sample/conversion operation"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 17th sample/conversion operation"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 18th sample/conversion operation"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 19th sample/conversion operation"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 20th sample/conversion operation"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 21th sample/conversion operation"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 22nd sample/conversion operation"/>
         <value>21</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 23rd sample/conversion operation"/>
         <value>22</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 24th sample/conversion operation"/>
         <value>23</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 25th sample/conversion operation"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 26th sample/conversion operation"/>
         <value>25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 27th sample/conversion operation"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 28th sample/conversion operation"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 29th sample/conversion operation"/>
         <value>28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 2nd sample/conversion operation"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 30th sample/conversion operation"/>
         <value>29</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 31th sample/conversion operation"/>
         <value>30</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 32nd sample/conversion operation"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 3rd sample/conversion operation"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 4th sample/conversion operation"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 5th sample/conversion operation"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 6th sample/conversion operation"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 7th sample/conversion operation"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 8th sample/conversion operation"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 9th sample/conversion operation"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every sample/conversion operation"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="ADRC" alias="FOSC/2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="ADRC" alias="RC clock"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="10"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="11"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="12"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="13"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="14"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="15"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="16"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="17"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="18"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="19"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="20"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="21"/>
         <value>21</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="22"/>
         <value>22</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="23"/>
         <value>23</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="24"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="25"/>
         <value>25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="26"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="27"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="28"/>
         <value>28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="29"/>
         <value>29</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="3"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="30"/>
         <value>30</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="31"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="4"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="5"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="6"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="7"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="8"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="9"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON4" settingAlias="ADDMAEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON4" settingAlias="ADDMAEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON4" settingAlias="DMABL" alias="Allocates 1 word of buffer to each analog input"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON4" settingAlias="DMABL" alias="Allocates 128 words of buffer to each analog input"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON4" settingAlias="DMABL" alias="Allocates 16 words of buffer to each analog input"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON4" settingAlias="DMABL" alias="Allocates 2 words of buffer to each analog input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON4" settingAlias="DMABL" alias="Allocates 32 words of buffer to each analog input"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON4" settingAlias="DMABL" alias="Allocates 4 words of buffer to each analog input"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON4" settingAlias="DMABL" alias="Allocates 64 words of buffer to each analog input"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON4" settingAlias="DMABL" alias="Allocates 8 words of buffer to each analog input"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS24" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS24" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS25" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS25" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS26" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS26" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS27" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS27" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCHS"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCHS123"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCON1"/>
         <value>33860</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCON2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCON3"/>
         <value>776</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCON4"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCSSH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCSSL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NA"/>
         <value>VREFL</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NB"/>
         <value>VREFL</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA"/>
         <value>AN4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB"/>
         <value>OA2/AN0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123NA"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123NB"/>
         <value>CH1=VREF-,CH2=VREF-,CH3=VREF-</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123SA"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHS123" settingAlias="CH123SB"/>
         <value>CH1=OA2/AN0,CH2=AN1,CH3=AN2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ADON"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ADSIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ASAM"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="DMABM"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="DONE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="FORM"/>
         <value>Absolute decimal result, unsigned, right-justified</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="MODE12"/>
         <value>12-bit</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SAMP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SIMSAM"/>
         <value>Sequential</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC"/>
         <value>TMR3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRCG"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="ALTS"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="BUFM"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="BUFS"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="CHPS"/>
         <value>1 Channel</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="CSCNA"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="NVCFG0"/>
         <value>AVSS</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="PVCFG"/>
         <value>AVDD</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI"/>
         <value>Generates interrupt after completion of every sample/conversion operation</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="ADCS"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="ADRC"/>
         <value>FOSC/2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON4" settingAlias="ADDMAEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON4" settingAlias="DMABL"/>
         <value>Allocates 1 word of buffer to each analog input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS24"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS25"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS26"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS27"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADI" settingAlias="enable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="DMT" name="USEDMT"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="DMT" name="customFDMTCNT"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="DMT" name="customFDMTIVT"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="DMT" name="customMasterSlaveViewerEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="DMT" registerAlias="DMTCON" settingAlias="ON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="DMT" registerAlias="DMTCON" settingAlias="ON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="DMT" registerAlias="DMTCLR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="DMT" registerAlias="DMTCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="DMT" registerAlias="DMTPRECLR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="DMT" registerAlias="DMTCLR" settingAlias="STEP2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="DMT" registerAlias="DMTCON" settingAlias="ON"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="DMT" registerAlias="DMTPRECLR" settingAlias="STEP1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ICD" name="customICS"/>
         <value>Communicate on PGEC3 and PGED3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ICD" name="customMasterSlaveViewerEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLKPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLKPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_FOSC"/>
         <value>138187500</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_FOSC2"/>
         <value>69093750</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_FRC"/>
         <value>7370000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_LPRC"/>
         <value>32768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_PRIMARY"/>
         <value>7370000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_USB"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="ClockSource"/>
         <value>FRC Oscillator</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="ClockSwitching"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FailSafe"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAutoTune"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockChange"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockEnable"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockFBDivisor"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockPostscaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockPostscaler2"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockPrescaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockSource"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxPll"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAvcoDivider"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureCANFDClock"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureClockChange"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureClockSource"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureClockSwitching"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureCodeGuard"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureFrcEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureFrcScaler"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureIESOUpdate"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureOscfDivisor"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureOscfdivEnable"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllCpuDivScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllDisplayScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllFeedbackDivisor"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllGraphicsSelect"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllPostScaler"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllScaler"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllTwoStagePostScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePoscErrataWorkaround"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefClkOutoutEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockDivSwitch"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockDivider"/>
         <value>NOTAVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockSource"/>
         <value>NOTAVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockTrim"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoOutputPinEnable"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureSoscClock"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureSoscEnable"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureUsb"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureVcoDivider"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FrcEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FrcPostscaler"/>
         <value>1:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FrcPostscalerClock"/>
         <value>7370000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="OSCPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="OSCPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllClock"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllDivisor"/>
         <value>1:75</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllPostscaler"/>
         <value>1:2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllPrescaler"/>
         <value>1:2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="Pll_Dependent_Clock_Switching"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_ENABLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_INPUT_FREQUENCY"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_RODIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_ROSEL"/>
         <value>FOSC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFOPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFOPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="Requested CAN Clock Frequency"/>
         <value>20000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="SCLKPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="SOSCPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="SOSCPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UI_OSCTUN_SETTING"/>
         <value>Center frequency</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllFeedbackDivisorOptions"/>
         <value>[1:33, 1:34, 1:35, 1:36, 1:37, 1:38, 1:39, 1:40, 1:41, 1:42, 1:43, 1:44, 1:45, 1:46, 1:47, 1:48, 1:49, 1:50, 1:51, 1:52, 1:53, 1:54, 1:55, 1:56, 1:57, 1:58, 1:59, 1:60, 1:61, 1:62, 1:63, 1:64, 1:65, 1:66, 1:67, 1:68, 1:69, 1:70, 1:71, 1:72, 1:73, 1:74, 1:75, 1:76, 1:77, 1:78, 1:79, 1:80, 1:81, 1:82, 1:83, 1:84, 1:85, 1:86, 1:87, 1:88, 1:89, 1:90, 1:91, 1:92]</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllPostscalerClock"/>
         <value>138187500</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllPostscalerOptions"/>
         <value>[1:8, 1:4, 1:2]</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllPrescalerClock"/>
         <value>3685000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllPrescalerOptions"/>
         <value>[1:9, 1:8, 1:7, 1:6, 1:5, 1:4, 1:3, 1:2]</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllfbDivisorClock"/>
         <value>276375000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="customClkOut"/>
         <value>OSC2 is general purpose digital I/O pin</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="customMasterSlaveViewerEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:128"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPOST" alias="1:2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPOST" alias="1:4"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPOST" alias="1:8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="10"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="11"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="12"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="13"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="14"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="15"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="16"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="17"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="18"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="19"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="20"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="21"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="22"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="23"/>
         <value>21</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="24"/>
         <value>22</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="25"/>
         <value>23</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="26"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="27"/>
         <value>25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="28"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="29"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="3"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="30"/>
         <value>28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="31"/>
         <value>29</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="32"/>
         <value>30</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="33"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="5"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="6"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="7"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="8"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE" alias="9"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/256"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="ROI" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="ROI" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="ACCSAT" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="ACCSAT" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="EDT" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="EDT" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="IF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="IF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="IPL3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="IPL3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="RND" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="RND" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="SATA" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="SATA" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="SATB" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="SATB" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="SATDW" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="SATDW" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="SFA" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="SFA" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="US" alias="mixed"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="US" alias="signed"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="US" alias="unsigned"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="VAR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="VAR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CF" alias="clock failure"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CF" alias="no clock failure"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CLKLOCK" alias="locked"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CLKLOCK" alias="unlocked"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="FRC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="FRCDIV"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="FRCPLL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="LPRC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="PRI"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="PRIPLL"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="LOCK" alias="in lock"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="LOCK" alias="out of lock"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="FRC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="FRCDIV"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="FRCPLL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="LPRC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="PRI"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="PRIPLL"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="OSWEN" alias="Request Switch"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="OSWEN" alias="Switch is Complete"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.047%"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.094%"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.141%"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.188%"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.235%"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.282%"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.329%"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.376%"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.423%"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.470%"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.517%"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.564%"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.611%"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.658%"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.705%"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.752%"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.799%"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.846%"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.893%"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.940%"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.987%"/>
         <value>21</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.034%"/>
         <value>22</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.081%"/>
         <value>23</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.128%"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.175%"/>
         <value>25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.222%"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.269%"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.316%"/>
         <value>28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.363%"/>
         <value>29</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.410%"/>
         <value>30</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.047%"/>
         <value>63</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.094%"/>
         <value>62</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.141%"/>
         <value>61</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.188%"/>
         <value>60</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.235%"/>
         <value>59</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.282%"/>
         <value>58</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.329%"/>
         <value>57</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.376%"/>
         <value>56</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.423%"/>
         <value>55</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.470%"/>
         <value>54</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.517%"/>
         <value>53</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.564%"/>
         <value>52</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.611%"/>
         <value>51</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.658%"/>
         <value>50</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.705%"/>
         <value>49</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.752%"/>
         <value>48</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.799%"/>
         <value>47</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.846%"/>
         <value>46</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.893%"/>
         <value>45</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.940%"/>
         <value>44</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.987%"/>
         <value>43</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.034%"/>
         <value>42</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.081%"/>
         <value>41</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.128%"/>
         <value>40</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.175%"/>
         <value>39</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.222%"/>
         <value>38</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.269%"/>
         <value>37</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.316%"/>
         <value>36</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.363%"/>
         <value>35</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.410%"/>
         <value>34</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.457%"/>
         <value>33</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center frequency"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Maximum frequency deviation"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Minimum frequency deviation"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="ADC1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="ADC1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="C1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="C1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="I2C1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="I2C1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="PWMMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="PWMMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T3MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T3MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T4MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T4MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T5MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T5MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC3MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC3MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC4MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC4MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC3MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC3MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC4MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC4MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="CMPMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="CMPMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="CTMUMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="CTMUMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="REFOMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="REFOMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="PWM1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="PWM1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="PWM2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="PWM2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="PWM3MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="PWM3MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD7" settingAlias="DMA0MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD7" settingAlias="DMA0MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="DMTMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="DMTMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="SENT1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="SENT1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="SENT2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="SENT2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSEL" alias="FOSC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSEL" alias="Primary Oscillator"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSSLP" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSSLP" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV"/>
         <value>12288</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON"/>
         <value>256</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD"/>
         <value>73</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD7"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE"/>
         <value>1:8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPOST"/>
         <value>1:2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="PLLPRE"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV"/>
         <value>FRC/1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="ROI"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="ACCSAT"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="DL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="EDT"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="IF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="IPL3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="RND"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="SATA"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="SATB"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="SATDW"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="SFA"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="US"/>
         <value>signed</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CORCON" settingAlias="VAR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CF"/>
         <value>no clock failure</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CLKLOCK"/>
         <value>unlocked</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC"/>
         <value>FRCDIV</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="LOCK"/>
         <value>out of lock</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC"/>
         <value>FRCPLL</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="OSWEN"/>
         <value>Switch is Complete</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN"/>
         <value>Center frequency</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PLLFBD" settingAlias="PLLDIV"/>
         <value>73</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="ADC1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="C1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="I2C1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="PWMMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T3MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T4MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T5MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC3MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC4MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC3MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC4MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="CMPMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="CTMUMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="REFOMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="PWM1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="PWM2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="PWM3MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD7" settingAlias="DMA0MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="DMTMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="SENT1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="SENT2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="RODIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSEL"/>
         <value>FOSC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSSLP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Interrupt Module" name="GlobalInterrupt"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name MCLR"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA0"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA2"/>
         <value>IO_RA2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA4"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB0"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB10"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB11"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB12"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB13"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB14"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB15"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB2"/>
         <value>channel_AN4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB4"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB5"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB6"/>
         <value>IO_RB6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB7"/>
         <value>SCK1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB8"/>
         <value>SDO1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB9"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Pin Module_CNIISRFunction"/>
         <value>ISR_Pin Module_CNI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA2"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB6"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet MCLR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc MCLR"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB10"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB11"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB12"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB13"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB14"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB15"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB5"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB6"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB7"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB8"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB9"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet MCLR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="packageId"/>
         <value>DIP28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA3"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA0" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA0" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA1" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA1" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA2" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA2" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA4" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA4" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB0" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB0" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB1" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB1" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB2" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB2" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB3" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB3" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB7" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB7" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB8" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB8" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB9" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB9" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENA" settingAlias="CNIEA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENA" settingAlias="CNIEA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENA" settingAlias="CNIEA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENA" settingAlias="CNIEA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENA" settingAlias="CNIEA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENA" settingAlias="CNIEA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENA" settingAlias="CNIEA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENA" settingAlias="CNIEA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENA" settingAlias="CNIEA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENA" settingAlias="CNIEA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB10" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB10" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB11" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB11" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB12" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB12" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB13" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB13" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB14" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB14" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB15" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB15" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB5" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB5" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB6" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB6" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB7" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB7" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB8" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB8" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB9" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB9" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB10" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB10" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB11" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB11" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB12" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB12" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB13" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB13" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB14" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB14" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB15" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB15" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB5" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB5" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB6" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB6" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB7" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB7" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB8" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB8" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB9" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB9" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ANSELA"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ANSELB"/>
         <value>524</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNENA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNENB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPDA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPDB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPUA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPUB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR11"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR12"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR18"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR19"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR22"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR23"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR26"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR3"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR37"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR38"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR39"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR44"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR45"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR7"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR8"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR3"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR4"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISA"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISB"/>
         <value>65087</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA0"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA1"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA2"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA4"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB0"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB1"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB2"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB3"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB7"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB8"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB9"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENA" settingAlias="CNIEA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENA" settingAlias="CNIEA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENA" settingAlias="CNIEA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENA" settingAlias="CNIEA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENA" settingAlias="CNIEA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNENB" settingAlias="CNIEB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA0"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA4"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB0"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB10"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB11"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB12"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB13"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB14"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB15"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB4"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB5"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB6"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB7"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB8"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB9"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR0" settingAlias="INT1R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR1" settingAlias="INT2R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR11" settingAlias="OCFAR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR12" settingAlias="FLT1R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR12" settingAlias="FLT2R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR18" settingAlias="U1RXR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR19" settingAlias="U2RXR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR22" settingAlias="SCK2R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR22" settingAlias="SDI2R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR23" settingAlias="SS2R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR26" settingAlias="C1RXR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR3" settingAlias="T2CKR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR37" settingAlias="SYNCI1R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR38" settingAlias="DTCMP1R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR39" settingAlias="DTCMP2R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR39" settingAlias="DTCMP3R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR44" settingAlias="SENT1R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR45" settingAlias="SENT2R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR7" settingAlias="IC1R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR7" settingAlias="IC2R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR8" settingAlias="IC3R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR8" settingAlias="IC4R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR0" settingAlias="RP20R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR0" settingAlias="RP35R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR1" settingAlias="RP36R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR1" settingAlias="RP37R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR2" settingAlias="RP38R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR2" settingAlias="RP39R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR3" settingAlias="RP40R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR3" settingAlias="RP41R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR4" settingAlias="RP42R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR4" settingAlias="RP43R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA0"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA1"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA2"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA3"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA4"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB0"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB1"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB10"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB11"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB12"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB13"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB14"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB15"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB3"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB4"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB5"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB6"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB7"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB8"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB9"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="BOR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="BOR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="EXTR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="EXTR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IDLE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IDLE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IOPUWR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IOPUWR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="POR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="POR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SLEEP" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SLEEP" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SWR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SWR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="TRAPR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="TRAPR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="WDTO" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="WDTO" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="RESET" registerAlias="RCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="BOR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="EXTR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="IDLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="IOPUWR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="POR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="SLEEP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="SWR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="TRAPR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="WDTO"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="ClockFrequency"/>
         <value>69093750.00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="DataModeSelect"/>
         <value>16 bit</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="OpMode"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="SCK1"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="SDI1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="SDO1"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="SPI1_SPFIISRFunction"/>
         <value>ISR_SPI1_SPFI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="SPI1_SPIIISRFunction"/>
         <value>ISR_SPI1_SPII</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="SS1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="CKE" alias="Active to Idle"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="CKE" alias="Idle to Active"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="CKP" alias="Idle:High, Active:Low"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="CKP" alias="Idle:Low, Active:High"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="DISSCK" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="DISSCK" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="DISSDO" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="DISSDO" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="MODE16" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="MODE16" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="MSTEN" alias="Master"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="MSTEN" alias="Slave"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="PPRE" alias="16:1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="PPRE" alias="1:1"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="PPRE" alias="4:1"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="PPRE" alias="64:1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="SMP" alias="End"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="SMP" alias="Middle"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="SPRE" alias="1:1"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="SPRE" alias="2:1"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="SPRE" alias="3:1"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="SPRE" alias="4:1"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="SPRE" alias="5:1"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="SPRE" alias="6:1"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="SPRE" alias="7:1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="SPRE" alias="8:1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="SSEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="SSEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="FRMDLY" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="FRMDLY" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="FRMEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="FRMEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="FRMPOL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="FRMPOL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="SPIBEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="SPIBEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="SPIFSD" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="SPIFSD" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SISEL" alias="SPI_INT_BUF_3_4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SISEL" alias="SPI_INT_BUF_EMPTY2NOT"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SISEL" alias="SPI_INT_ENHBUF_1SPOT"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SISEL" alias="SPI_INT_ENHBUF_EMPTY"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SISEL" alias="SPI_INT_LAST_WORD_READ"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SISEL" alias="SPI_INT_SPIRBF"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SISEL" alias="SPI_INT_SPITBF"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SISEL" alias="SPI_INT_TRMT_COMPLETE"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIBEC" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIBEC" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIRBF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIRBF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIROV" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIROV" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPISIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPISIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPITBF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPITBF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SRMPT" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SRMPT" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SRXMPT" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SRXMPT" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="SPI1" registerAlias="SPIBUF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="SPI1" registerAlias="SPICON1"/>
         <value>1343</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="SPI1" registerAlias="SPICON2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="SPI1" registerAlias="SPISTAT"/>
         <value>32780</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPFI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPFI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPFI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPFI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPIBUF" settingAlias="SPIBUF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="CKE"/>
         <value>Active to Idle</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="CKP"/>
         <value>Idle:Low, Active:High</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="DISSCK"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="DISSDO"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="MODE16"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="MSTEN"/>
         <value>Master</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="PPRE"/>
         <value>1:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="SMP"/>
         <value>Middle</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="SPRE"/>
         <value>1:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON1" settingAlias="SSEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="FRMDLY"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="FRMEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="FRMPOL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="SPIBEN"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="SPIFSD"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPII" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPII" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPII" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPII" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SISEL"/>
         <value>SPI_INT_SPIRBF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIBEC"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIEN"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIRBF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIROV"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPISIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPITBF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SRMPT"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SRXMPT"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="IPL1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="IPL2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="IPL3"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="IPL4"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="IPL5"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="IPL6"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="IPL7"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1" alias="OFF"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="IPL1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="IPL2"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="IPL3"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="IPL4"/>
         <value>48</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="IPL5"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="IPL6"/>
         <value>80</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="IPL7"/>
         <value>96</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2" alias="OFF"/>
         <value>112</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="ALTI2C1" alias="OFF"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="ALTI2C1" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="PWMLOCK" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="PWMLOCK" alias="ON"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDMT" settingAlias="DMTEN" alias="DISABLE"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDMT" settingAlias="DMTEN" alias="ENABLE"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS" alias="NONE"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS" alias="PGx1"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS" alias="PGx2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS" alias="PGx3"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="FCKSM" alias="CSDCMD"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="FCKSM" alias="CSECMD"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="FCKSM" alias="CSECME"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="IOL1WAY" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="IOL1WAY" alias="ON"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="OSCIOFCN" alias="OFF"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="OSCIOFCN" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="PLLKEN" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="PLLKEN" alias="ON"/>
         <value>256</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCMOD" alias="EC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCMOD" alias="HS"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCMOD" alias="NONE"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCMOD" alias="XT"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="FRC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="FRCDIV"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="FRCDIV16"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="FRCPLL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="LPRC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="PRI"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="PRIPLL"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="IESO" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="IESO" alias="ON"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BOREN0" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BOREN0" alias="ON"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="AIVTDIS" alias="DISABLE"/>
         <value>32768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="AIVTDIS" alias="ENABLE"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BSEN" alias="OFF"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BSEN" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BSS" alias="DISABLED"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BSS" alias="HIGH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BSS" alias="STNDRD"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BWRP" alias="OFF"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BWRP" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CSS" alias="DISABLED"/>
         <value>3584</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CSS" alias="ENHNCD"/>
         <value>2048</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CSS" alias="HIGH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CSS" alias="STNDRD"/>
         <value>3072</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CWRP" alias="OFF"/>
         <value>256</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CWRP" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="GSS" alias="DISABLED"/>
         <value>192</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="GSS" alias="HIGH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="GSS" alias="STNDRD"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="GWRP" alias="OFF"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="GWRP" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN" alias="ON"/>
         <value>96</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN" alias="ON_DIS_SLEEP"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN" alias="ON_SWDTEN"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWPSA" alias="PR128"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWPSA" alias="PR32"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS1024"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS128"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS16384"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS2048"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS256"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS32768"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS4096"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS512"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS8192"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTWIN" alias="WIN25"/>
         <value>768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTWIN" alias="WIN37"/>
         <value>512</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTWIN" alias="WIN50"/>
         <value>256</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTWIN" alias="WIN75"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WINDIS" alias="OFF"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WINDIS" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FALTREG"/>
         <value>119</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FBSLIM"/>
         <value>8191</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FDEVOPT"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FDMT"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FDMTCNTH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FDMTCNTL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FDMTINTVH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FDMTINTVL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FICD"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FOSC"/>
         <value>355</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FOSCSEL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FPOR"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FSEC"/>
         <value>36847</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FWDT"/>
         <value>927</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT1"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FALTREG" settingAlias="CTXT2"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FBSLIM" settingAlias="BSLIM"/>
         <value>8191</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="ALTI2C1"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="PWMLOCK"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDMT" settingAlias="DMTEN"/>
         <value>DISABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDMTCNTH" settingAlias="DMTCNTH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDMTCNTL" settingAlias="DMTCNTL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDMTINTVH" settingAlias="DMTIVTH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDMTINTVL" settingAlias="DMTIVTL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS"/>
         <value>PGx3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="FCKSM"/>
         <value>CSECMD</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="IOL1WAY"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="OSCIOFCN"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="PLLKEN"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCMOD"/>
         <value>NONE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC"/>
         <value>FRCPLL</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="IESO"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BOREN0"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="AIVTDIS"/>
         <value>DISABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BSEN"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BSS"/>
         <value>DISABLED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="BWRP"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CSS"/>
         <value>DISABLED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CWRP"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="GSS"/>
         <value>DISABLED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="GWRP"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWPSA"/>
         <value>PR128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS"/>
         <value>PS32768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTWIN"/>
         <value>WIN25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WINDIS"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="T3CK"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="TMR3_TIISRFunction"/>
         <value>ISR_TMR3_TI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="TimerFrequency"/>
         <value>69093750</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="actualPeriod"/>
         <value>0.0000667065</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="callBackRate"/>
         <value>0.0000667065</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="clockSourceSelect"/>
         <value>FOSC/2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="combinedTimer"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="customPR"/>
         <value>4608</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="inputMode"/>
         <value>periodMode</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="localClockFreq"/>
         <value>69093750</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="maxPeriod"/>
         <value>0.0009485084</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="minPeriod"/>
         <value>0.0000000289</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="prescaleDivisor"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="prescaledFreq"/>
         <value>69093750.00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="requestedPeriod"/>
         <value>0.0000667</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="tickerFactor"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="timerBitMode"/>
         <value>16 Bit</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="timerExtPinSelection"/>
         <value>FALSE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR3" name="timerMaxCount"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TCKPS" alias="1:1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TCKPS" alias="1:256"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TCKPS" alias="1:64"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TCKPS" alias="1:8"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TCS" alias="FOSC/2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TCS" alias="T3CK"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TGATE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TGATE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TSIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TSIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="TMR3" registerAlias="PR"/>
         <value>4608</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="TMR3" registerAlias="TCON"/>
         <value>32768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="TMR3" registerAlias="TMR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR3" registerAlias="PR" settingAlias="PR"/>
         <value>4608</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TCKPS"/>
         <value>1:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TCS"/>
         <value>FOSC/2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TGATE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TON"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR3" registerAlias="TCON" settingAlias="TSIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR3" registerAlias="TI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR3" registerAlias="TI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR3" registerAlias="TI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR3" registerAlias="TI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR3" registerAlias="TMR" settingAlias="TMR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="ClockInput"/>
         <value>32768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="TimerPeriod"/>
         <value>128.000s</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="clockSourceSelect"/>
         <value>CLOCK_LPRC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="customMasterSlaveViewerEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="customViewerUpdate"/>
         <value>disabled</value>
      </entry>
   </tokenMap>
   <generatedFileHashHistoryMap class="java.util.TreeMap">
      <entry>
         <file>main.c</file>
         <hash>209e334a3becc2d15506f71cd78fc5ea3be9aad0b45a2b6ab0cd3c61f72122be</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\adc1.c</file>
         <hash>8db5364f097546482c386e75d57292d5a1134b47b91beff7c7bb1f9266574bd0</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\adc1.h</file>
         <hash>00804ed3dad51fdef241a083428b4c646a5a3cedd0a768130549b4cd22ca28c3</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\adc_module_features.h</file>
         <hash>ec9c64046727a536338d87d30b3ccabcb9f9a6c9d3854b0877c18674f67be627</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\clock.c</file>
         <hash>838c6f46712edfef83959f1d04b71d3b74dc9c63dcd5ba21b3249b59f60718b3</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\clock.h</file>
         <hash>0ccf1ac17dd9e27f7506c683bb00de156c1644848f6e0fa1d3405288d0f58dd3</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\interrupt_manager.c</file>
         <hash>f2097a464f5da72ebe60f0ef38bea2be70734cef6745c664475fd0426e5bc590</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\interrupt_manager.h</file>
         <hash>61cea081aaa87511d1dc8529b1af1afa975b2f7a97455b176e9a64322e5008c0</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\mcc.c</file>
         <hash>1d55648f95fe132e3ac489587a7bbf3cb0e679fbc6ee10be43ec35411e97e550</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\mcc.h</file>
         <hash>28063936f266af6649056b7675553e4a9221b708d2b7854fca506a10b181225c</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pin_manager.c</file>
         <hash>89f2bbcc62b1ca65c91ac792b7837a6414224b6d6391daf793ec17788bff3643</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pin_manager.h</file>
         <hash>4f4d836de113e4dc5c8cfdbc9c32c6a73d553344f2efd6029fcc2cd7284ff735</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\reset.c</file>
         <hash>07eba371281487cf4899585105edfa92d15e018ed9bdf07f5306a3f34cec1970</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\reset.h</file>
         <hash>f12e826679b39c3549507825f7c342afa3ff89c2205af5d244f9c69ca2b836bb</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\reset_types.h</file>
         <hash>45c45acfb6b403b208d2a16aaaf8ff74291e73ffac5cd606ab911e141447835c</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\spi1.c</file>
         <hash>5b778d3d17142815cf4f6a7990fe3a6d97e0133c2ce2932fd5286fc6d0634428</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\spi1.h</file>
         <hash>b9829f53e3410587c5cc81d4ae8653c1d8976f8329221639b4c9140cb7b10557</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system.c</file>
         <hash>eeda46a53ca0becbd80e09a8eb396febbd0c6a99cb2fcc9de2567049d40cfa50</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system.h</file>
         <hash>9b5abcd07500c9170275b20d1aed08595254c381f8762fdc6e3edfe03e65925f</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system_types.h</file>
         <hash>d79f58835a602a5f8b07845bccf325ed5974450342050d8de9e5819f83aa1808</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\tmr3.c</file>
         <hash>3f4a3644e4250f23adc13b77b77298bf81df2fb3ce35945bc9762ca6ed769986</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\tmr3.h</file>
         <hash>9177994317cb1096786fada4cb9ad0fe2693a304734a0e4cae73c6e847abe8fe</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\traps.c</file>
         <hash>466071b6182e23a156b191e6ee063645f868945a584e9c287004f4a5ef4416ca</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\traps.h</file>
         <hash>eb4e6c6d15278b2bc272ccf8a3788894f717d912cbe908a885ef211f54558538</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\watchdog.h</file>
         <hash>b4959606f68dd3eba0b1e6806c7eee0e08b4b047014c2b7f2a72e8524b9ec709</hash>
      </entry>
   </generatedFileHashHistoryMap>
</config>